Release Notes

A picture containing indoor, table, small, sitting

Description automatically generated

Table of Contents

[Version 1.0.0 3](#_Toc53091703)

[Version 1.1.0 3](#_Toc53091704)

[Version 1.2.0 3](#_Toc53091705)

# Version 1.0.0

|  |  |
| --- | --- |
| **Version** | v1.0.0 |
| **Author** | Samuel Netherway |
| **Release Date** | 18/08/2020 |
| **Intended Users** | All Users |
| **Changes** | Stock config. |
| **Important Details** | Frequencies should not be used without the correct licencing. |

# Version 1.1.0

|  |  |
| --- | --- |
| **Version** | v1.1.0 |
| **Author** | Samuel Netherway |
| **Release Date** | 18/08/2020 |
| **Intended Users** | All Users |
| **Changes** | * Added UK Licence Free Radio Frequencies on memory channels 1 to 8. * Removed all channel frequency pre-sets, i.e. only 1 through 8 are used. |
| **Important Details** | UK Licence Free Frequencies List:   * Channel 1: 446.00625 * Channel 2: 446.01875 * Channel 3: 446.03125 * Channel 4: 446.04375 * Channel 5: 446.05625 * Channel 6: 446.06875 * Channel 7: 446.08125 * Channel 8: 446.09375   All channels are pre-set to transmit on low power. |

# Version 1.2.0

|  |  |
| --- | --- |
| **Version** | v1.2.0 |
| **Author** | Samuel Netherway |
| **Release Date** | 08/10/2020 |
| **Intended Users** | All Users |
| **Changes** | Added UK PMR 446 frequencies to channels 1 through 16 and set to transmit on low power by default. |
| **Important Details** |  |